

**Vermont Electric Cooperative, Inc. NEW SERVICE APPLICATION**

Attn: Operations & Engineering Coordinator

42 Wescom Road Toll Free: 1-800-832-2667 ext. 1117

Johnson, VT 05656-9717 Telephone: 802-635-2331 ext. 1117

Email: scheduling@vermontelectric.coop Fax: 802-635-4210

Name: Last, First, Middle Initial Co-Applicant Name: Last, First, Middle Initial

Mailing address Town State Zip

**Home Phone** Work Phone Cell Phone

**Email Address**

**Building Site Physical Address**  **Town**

**Check appropriate box(s):**

**Type of Service:** **Size of Service: Wires: Primary**

 Residential 100amp Overhead

 Duplex 200amp Underground

 Garage 400amp

 Job Trailer other, specify: **Secondary**

Commercial Overhead

Mobile Home Secondary Job Trailer

Farm, specify:

 **Distance from nearest VEC pole or vault to building site:** Footage

 **Contractor:**

 General Contractor Telephone

 Electrician Telephone

**TEMPORARY ELECTRIC SERVICE**

I agree to provide the following:

1) To provide, erect or install an adequate distribution panel and to maintain such a panel in a weatherproof condition.

2) To install a 3 wire circuit (per NEC) to the distribution panel, which shall be sized to the amperage of the main disconnect, as specified above.

3) To install 2 copper ground rods at the distribution panel, such rods to have at least the minimum dimensions of 8 feet in length and ½ inch in diameter.

4) To install ground fault protection (see drawing) on all 120-volt circuits going out of the distribution panel.

5) To accept full responsibility to examine and inspect daily, prior to use, all electrical tools, extension cords, and equipment.

6) To perform all installation in full compliance with the requirements of the National Electric Code (NEC) of the National Board of Fire Underwriters, together with any state or local electric codes or regulations, where applicable.

7) To have and hold VEC harmless from, and to indemnify VEC against any and all claims, actions, or suits for injury, damage, or loss of persons or property however caused, which may arise or be alleged to have arisen in connection with the furnishing of electric service under this agreement.

8) To make advance payment for labor and expense of performing the temporary connection and for all material, including salvageable material, when applicable, and as required by the filed tariff of VEC.

9) All energy used during the period for the temporary service as provided is to be billed to the above address at the application rate set forth in VEC’s tariff rate schedule.

10) Application valid for 6 months from date of application, after which VEC will review and disconnect or extend the application date.

Please refer to appropriate drawing for either the overhead or underground temporary service that will be provided to you by the Utility Designer.

If you are requesting a temporary service please initial that you have read the above Temporary Electric Service information and will forward to your electrician or general contractor.

 Attach either a site plan or a hand drawn sketch of the layout of the lot (i.e.- driveway, septic system,

 water well, etc.).

 Attach the appropriate load sheet for the type of service requesting (choose link):

 To be created

**Member Service Agreement**

By Vermont Electric Cooperative, Inc.’s (VEC) filed tariff, the new member is allowed the installation cost credit of 100 feet of overhead service. If the new member requires an extension longer than 100 feet of overhead, by VEC’s filed tariff, the member will be required to contribute towards the cost of the extension according to the appropriate rate schedule.

In addition, for any line extension, the new member is required to furnish at their cost all required tree clearing, Right of Way procurements, permits, trenching, conduit and backfill for underground installations, if required. Any work performed by VEC on behalf of a member associated with line extensions, relocations, upgrades, or equipment replacements, which are not specifically covered by the charges contained in this tariff, will be billed to the member at VEC’s actual costs of performing the service.

If the new line extension secondary will cross a neighbor’s property it is the **member’s** responsibility for obtaining approval from the neighbor for this line.

Furnished by VEC:

1. All necessary materials with overhead line extension(s), pole(s), and riser(s), if required, and meter(s) installed; costs paid by member in accordance with the filed tariffs
2. Application packet of forms to be completed by member
3. Copy of VEC filed electric service Line Extension Policy, line extension charges and VEC’s Electric Service Requirements

Furnished by Member:

1. Completed application packet including signed Application for Service and/or Additional Service and any right of way easements
2. Member shall install a minimum of four stakes to show the approximate location of proposed building. The cost of the additional utility designing required due to relocation or re-orientation of proposed building or buildings after the original site survey will be borne in full by the member
3. All material furnished and installed by the member shall comply with the latest edition of National Electrical Safety Code (NESC) and VEC’s Electric Service Requirements (see construction drawings provided in packet)
4. One of the following:

 Overhead:

1. Cost of all right of way clearing
2. Meter socket on building (provide by owner’s electrician)
3. Cost for all extensions over 100 feet in length according to attached schedule

 Underground Secondary

1. Cost of all right of way clearing
2. All trenching, backfilling, conduit, wire, meter sockets, and grounding system (per NESC)
3. Cost for all extensions over allowable service credit according to attached rate schedule
4. Stub pole or 10’ x 6” x 6” pressure treated post, set 4’ in ground, which member agrees to install and maintain (see construction drawings), or two stub poles w/ 5/4” pressure treated back-board for multiple services

 Underground Primary

1. Cost of all right of way clearing
2. All trenching, backfilling, conduits and vaults as required
3. Cost of primary underground extension
4. Pull line capable of 500 lbs. pull strength

 **NOTE:** Primary (wire conductor) to be provided by VEC

Member Changes:

1. Members shall give proper notice to VEC of any increase or decrease proposed in load of 100 amps or greater
2. Members and their Contractors are prohibited from modifying service equipment, without the notification and consent of VEC, and, when required, the appropriate State or Local Inspection Authority. Examples of modifications that require prior notification and consent are:

1) Replacing, or adding, a main panel for the purpose of increasing capacity.

2) Other actions that may create safety concerns, NESC violations, equipment overloads, or be contradictory to these Service Requirements or VEC Tariffs

1. Failure on the part of the member to give notice as provided above shall render them liable for any damages to meters, transformers, wires, and associated apparatus of VEC resulting from the use of increased or changed load. These costs will be in excess of those the member would have borne if they had contacted VEC in advance of these changes

We the undersigned, hereby agree to the above requirements and conditions for electric service. We understand that before construction will be started payment for the costs of the extension must be paid in full. We also understand that initial billing for construction may be subject to “true up” when job is completed. This will be a **line item** (14200) on the initial construction bill. This means an additional bill may be mailed to you at the end of your job and payment is expected.

![C:\Users\ddurivage\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\CR3DFVYC\check-mark[1].png]() ![C:\Users\ddurivage\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\CR3DFVYC\check-mark[1].png]()

 Applicant’s Electronic Signature Date Co-Applicant’s Electronic Signature

 **INVOICE**

Attn: Operations & Engineering Coordinator

42 Wescom Rd

Johnson VT 05656

Item # Description Qty Price Total Due

142.25 Engineering Fee 1 $250.00

  **$250.00**

Payments accepted up to $2,500.00 if using a credit card: 

**Note:** A $250.00 fee will be charged for each additional site visit(s) when required.

 Initial billing for construction may be subject to “true up” when job is completed. This will be a **line item** on the construction bill. This means an additional bill may be mailed to you at the end of your jo